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SPECIFICATIONS - SECTION 10 22 26 SUPPORT SYSTEM FOR OPERABLE PARTITIONS

Part 1 – General

1.1 Description

A. General:
1. Furnish and install support system for operable partitions.  Provide all labor, materials, tools, equipment, and services for support system in accordance with provisions of contract documents.

1.2 Related work by others

A. Preparation of opening will be by General Contractor.  Any deviation of site conditions contrary to approved shop drawings must be called to the attention of the architect.

[bookmark: _GoBack1]B. All structural bracing, track enclosures, surrounding insulation, and sound baffles as required in 1.4 Quality Assurance.

C. Paint or otherwise finishing all trim and other materials adjoining head and jamb of support system.

1.3 Submittals

A. Complete shop drawings are to be provided prior to fabrication indicating construction and installation details.  Shop drawings must be submitted within 60 days after receipt of signed contract.

1.4 Quality Assurance

A. Installation shall be performed by an installer certified by the manufacturer.

B. Preparation of the opening shall conform to the criteria set forth by ASTM E557 Standard Practice for Architectural Application and Installation of Operable Partitions.

1.5 Product delivery, storage, and handling

A. Proper storage of support system before installation, and continued protection during and after installation will be the responsibility of the General Contractor.

1.6 Warranty

A. Support system shall be guaranteed for a period of two years. This guarantee is against defects in material or workmanship of manufacturer’s product, excluding abuse.

Part 2 – Products

2.1 Manufacturers

A. Manufacturers: Subject to compliance with requirements, provide products by the following:
1. Moderco Inc.

2.2 Products

A. Atlas support system.

B. Type of horizontal section (select one):
	1. Single steel beam.
2. 3-section steel beam. (Optional)

2.3 Materials

A. Components:
1. Structural components shall be factory fabricated with steel and aluminum. Moderco support system is attached to the building structure for lateral support only. The load of the support and partition systems is supported by the column support tubes. 
2. Base End Tube and I-Beam Sections. Bolt together structure has aluminum tubes and steel I-beam sections with integral track attachments points. 
3. Column Support Tubes. Column support tubes shall be 2 5/8” x 4” (67mm x 100mm) aluminum. Column support tubes shall be attached to the I-beam with steel brackets and bolts. Column support tubes shall be anchored to the floor with concealed fasteners utilizing a base plate. 
4. Support bracing provides operational stability to the Moderco support system and shall be set at each column support tube and centered in each I-beam section. Blocking for truss bracing to be provided by others in accordance with the manufacturer’s specifications.

B. Atlas support system manufactured by Moderco:
1. The I-beam is to be shipped in a single piece covering the entire span of the support. 
2. The I-beam is to be shipped in sections and assembled on site for custom assembly which meets site conditions. Maximum weight of any component should not exceed 300 Lbs (140 kg). (Optional)

C. Base plate:
1. Concealed base plate for each column support Tube limits the direct load on the floor to 400 psi maximum.

Part 3 – Execution

3.1 Installation

A. The complete installation of the support system shall be by an authorized factory-trained installer and be in strict accordance with the approved shop drawings and manufacturer’s installation instructions.

B. Assemble and install Moderco support system on site for custom assembly which meets site conditions. Adjust aluminum columns and steel beam assemblies to meet requirements specific to this project.

3.2 Cleaning

A. Clean component surfaces upon completing installation of support system to remove dust, dirt, and other foreign materials according to manufacturer’s instructions.

B. Packing and other installation debris shall be removed from the job site.

3.3 Examination

A. Examine flooring, Moderco support system, and opening, with installer present, for compliance with requirements for installation tolerances and other conditions affecting performance of
operable partitions. Proceed with installation of operable partitions only after unsatisfactory conditions have been corrected.
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